Table 1: Sources used for checking the photometric calibration and the relative response calibration of the LWS grating and Fabry Perot subsystems. The primary source for the grating flux calibration is Uranus, the other sources have been observed regularly for monitoring purposes. FG: Fixed Grating; FP: Fabry Perot.

Absolute Flux Calibration of LWS: checking and monitoring

Source Type Observation Uranus Planet FG position On and Off source and full scan Neptune Planet FG position On and Off source and full scan 1 Ceres Asteroid FG position On and Off source 2 Pallas Asteroid FG position On and Off source 4 Vesta Asteroid FG position On and Off source Arcturus Star FG position On and Off source and full scan Aldebaran Star FG position On and Off source and full scan Gamma Dra Star FG position On and Off source S106 HII region FG position and full scan G298.288 HII region FG position and full scan NGC 6543 Planetary Nebula full grating scan NGC 7027 Planetary Nebula full grating scan

FP throughput correction (transmission x resolution element) Mars Planet FP scans with fixed grating (mix mode)