Table 1: Summary of primary SWS Astronomical Calibration Standards

Source Alias Spectral Calibration Range Type Type^a [μm] HR4763^b γ Cru M4 III f 12−35 HR5340^b α Boo K1bCN III FB 2.4−45.2 HR6705 γ Dra K5 III FR 2.4−28 HR7001^c α Lyr A0 V fR 2.4−16 HR7310 δ Dra G9 III fl 2.4−45.2 NML Cyg^d IRC+10448 M6 IIIe fBR 16−45.2

Notes:

a: Calibration types: F = primary flux calibration source; f = secondary flux calibration source; l = linearity check;

B = beam profile calibration source; R = RSRF calibration source.

b: limited visibility c: Vega d: tertiary calibrator (see text)