Improvements to the LWS internal illuminator data processing

S.D. Sidher^{1,2}, B. M. Swinyard^2, A.S. Harwood^2, T.L. Lim^2

1Physics Department, Queen Mary, University of London, Mile End Road, London E1 4NS, UK 2Space Science and Technology Department, Rutherford Appleton Laboratory, CLRC, Chilton, Didcot, Oxon, OX11 OQX, UK

The use of a revised algorithm for processing internal illuminator flash data has led to significant improvements in the LWS calibration. The application of this new technique, which is implemented in the OLP 10 pipeline, will be explained and illustrative examples given.